**Run Project from microSD to NEXTION LCD**

1. After you design GUI click **Debug**
2. Click **Compile** and please check if your programs have a warning
3. Click **File**
4. Click **Open build folder**
5. Or you can access in Windows 10

**C:\Users\User\AppData\Roaming\Nextion Editor\bianyi**

1. **Copy .tft** files into your microSD
2. **Plug in** microSD to NEXTION
3. **Plug in** NEXTION to PC with USB cable
4. NEXTION will update and show success text
5. **Plug out** NEXTION USB cable from PC
6. **Plug out** microSD from NEXTION
7. **Plug in** NEXTION to PC with USB cable